# Intel Partition Table

### From CGSecurity

## How is the Partition Table written ?

CHS (Cylinder, Head, Sector) values are limited by a set number of bits for each value in the 16-byte partition table entries to: 1023,254,63. So LBA and CHS values can't be equal for HD bigger than 8GB.

There are two ways to store the CHS value:

- first way

     convert LBA to CHS,
     store (cylinder & 0x3FF, head & 0xFF, sector & 0x3F)

It's what Partition Magic does (prior to version 8.0?).

- second way

     convert LBA to CHS
     if cylinder <= 1023,
       store (cylinder & 0x3FF, head & 0xFF, sector & 0x3F)
     else
       store (1023, max_head & 0xFF, max_sector & 0x3F)

This is what Linux fdisk and TestDisk do.

When TestDisk checks the partition table, it considers both ways may be correct. But the second way is better because start CHS is always lower or equal to end CHS.

Example: A hard disk's logical geometry is 255 heads per cylinder and 63 sectors per head. A partition begins at LBA=46781280 or CHS=2912,0,1. This partition ends at 3072,254,63.

- First way:

     start:  864,  0, 1
     end:      0,254,63

- Second way:

     start: 1023,254,63
     end:   1023,254,63

NB: 1023 = 0x3FF (1023*255+254)*63+63-1=16450559 (2912*255+ 0)*63+ 1-1=46781280

Partition Magic (before version 8.0?) considered the second way as invalid; even though it's an agreed upon standard. TestDisk handles both without complaining.

Return to TestDisk main page

Categories: Data Recovery

##### Data Recovery

- TestDisk
- PhotoRec
- Download